|  |  |  |
| --- | --- | --- |
| **VERANDAH SCREEN OPENING MEASURING 2120×4530mm** | | |
|  |  | Date: 01/07/2021 |
|  |  |  |

|  |  |  |  |
| --- | --- | --- | --- |
| **Qty** | **Description** | **Unit Price (US$)** | **Total (US$)** |
| 5 lengths | Bordering 30×30 Square tube | 11 | 55 |
| 16 lengths | Uprights 20×20 Square Tube | 8 | 128 |
| 4 lengths | Flat bar 20mm | 4 | 16 |
| 1 Pair | Butterfly Hinges | 4 | 4 |
| 2 | Cutting & Grinding Disks | 3 | 6 |
|  | Lock rest plates |  | 4 |
| 1 liter | Red oxide |  | 15 |
|  | Thinners |  | 5 |
|  | Electrodes 2.15mm |  | 10 |
| 1 | 14mm round bar |  | 5 |
|  | Transport |  | 15 |
|  |  |  |  |
|  |  | Subtotal | 263 |
|  |  | Labor | 110 |
|  |  | Total | 373 |